./build.sh init
processing option: init

You're building on Linux
Lunch menu...pick a combo:

1. BoardConfig-ab-base.mk
2. BoardConfig-dr4-rk3566-buildroot.mk
3. BoardConfig-dr4-rk3566-debian.mk
4. BoardConfig-dr4-rk3566-ubuntu.mk
5. BoardConfig-dr4-rk3568-buildroot.mk
6. BoardConfig-dr4-rk3568-debian.mk
7. BoardConfig-dr4-rk3568-ubuntu.mk
8. BoardConfig-multi-dtb-nano-box-rk3566-buildroot.mk
9. BoardConfig-multi-dtb-nano-box-rk3566-debian.mk
10. BoardConfig-multi-dtb-nano-box-rk3566-ubuntu.mk
11. BoardConfig-multi-dtb-nano-box-rk3568-buildroot.mk
12. BoardConfig-multi-dtb-nano-box-rk3568-debian.mk
13. BoardConfig-multi-dtb-nano-box-rk3568-ubuntu.mk
14. BoardConfig-multi-dtb-rp-box-rk3566-buildroot.mk
15. BoardConfig-multi-dtb-rp-box-rk3566-debian.mk
16. BoardConfig-multi-dtb-rp-box-rk3566-ubuntu.mk
17. BoardConfig-nano-box-rk3566-buildroot.mk
18. BoardConfig-nano-box-rk3566-debian.mk
19. BoardConfig-nano-box-rk3566-ubuntu.mk
20. BoardConfig-nano-box-rk3568-buildroot.mk
21. BoardConfig-nano-box-rk3568-debian.mk
22. BoardConfig-nano-box-rk3568-ubuntu.mk
23. BoardConfig-nano-rk3566-buildroot.mk
24. BoardConfig-nano-rk3566-debian.mk
25. BoardConfig-nano-rk3566-ubuntu.mk
26. BoardConfig-nano-rk3568-buildroot.mk
27. BoardConfig-nano-rk3568-debian.mk
28. BoardConfig-nano-rk3568-ubuntu.mk
29. BoardConfig-pro-rk3566-buildroot.mk
30. BoardConfig-pro-rk3566-debian.mk
31. BoardConfig-pro-rk3566-ubuntu.mk
32. BoardConfig-pro-rk3568-buildroot.mk
33. BoardConfig-pro-rk3568-debian.mk
34. BoardConfig-pro-rk3568-ubuntu.mk
35. BoardConfig-rp-box-rk3566-buildroot.mk
36. BoardConfig-rp-box-rk3566-debian.mk
37. BoardConfig-rp-box-rk3566-ubuntu.mk
38. BoardConfig-rp-box-rk3568-buildroot.mk
39. BoardConfig-rp-box-rk3568-debian.mk
40. BoardConfig-rp-box-rk3568-ubuntu.mk
41. BoardConfig-rp-rk3566-buildroot.mk
42. BoardConfig-rp-rk3566-debian.mk
43. BoardConfig-rp-rk3566-ubuntu.mk
44. BoardConfig-rp-rk3568-buildroot.mk
45. BoardConfig-rp-rk3568-debian.mk
46. BoardConfig-rp-rk3568-ubuntu.mk
47. BoardConfig-security-base.mk
Which would you like? [0]: 32
switching to board: /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/device/rockchip/rk356x/BoardConfig-pro-rk3568-buildroot.mk
rpdzkj@90:~/ninth/yushun/rk3566-rk3568-linux$ source envsetup.sh rockchip_rk3568
Top of tree: /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux
===========================================

#TARGET_BOARD=rk3568
#OUTPUT_DIR=output/rockchip_rk3568
#CONFIG=rockchip_rk3568_defconfig

===========================================
make: Entering directory '/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot'
  GEN     /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/Makefile
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/build/defconfig_hook.py -m /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/configs/rockchip_rk3568_defconfig /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig
BR2_DEFCONFIG='' KCONFIG_AUTOCONFIG=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/build/buildroot-config/auto.conf KCONFIG_AUTOHEADER=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/build/buildroot-config/autoconf.h KCONFIG_TRISTATE=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/build/buildroot-config/tristate.config BR2_CONFIG=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.config HOST_GCC_VERSION="9" BASE_DIR=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568 SKIP_LEGACY= BR2_DEFCONFIG=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/configs/rockchip_rk3568_defconfig /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/build/buildroot-config/conf --defconfig=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig Config.in
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:259:warning: override: reassigning to symbol BR2_PACKAGE_ROCKCHIP_MPP
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:260:warning: override: reassigning to symbol BR2_PACKAGE_ROCKCHIP_MPP_ALLOCATOR_DRM
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:262:warning: override: reassigning to symbol BR2_PACKAGE_ROCKCHIP_RGA
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:287:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_GOOD_PLUGIN_RTP
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:288:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_GOOD_PLUGIN_RTPMANAGER
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:289:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_GOOD_PLUGIN_RTSP
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:295:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_BASE_PLUGIN_VIDEORATE
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:296:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_BASE_PLUGIN_VORBIS
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:297:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_BASE_PLUGIN_OGG
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:300:warning: override: reassigning to symbol BR2_PACKAGE_BLUEZ5_UTILS
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:319:warning: override: reassigning to symbol BR2_PACKAGE_ROCKCHIP_TEST
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:322:warning: override: reassigning to symbol BR2_PACKAGE_RKWIFIBT
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:361:warning: override: reassigning to symbol BR2_PACKAGE_RKSCRIPT_IODOMAIN
#
# configuration written to /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.config
#
make: Leaving directory '/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot'
rpdzkj@90:~/ninth/yushun/rk3566-rk3568-linux$ ./build.sh
processing option: allsave
============================================
TARGET_ARCH=arm64
TARGET_PLATFORM=rk356x
TARGET_UBOOT_CONFIG=rk3568
TARGET_SPL_CONFIG=
TARGET_KERNEL_CONFIG=rockchip_linux_defconfig
TARGET_KERNEL_DTS=pro-rk3568
TARGET_TOOLCHAIN_CONFIG=
TARGET_BUILDROOT_CONFIG=rockchip_rk3568
TARGET_RECOVERY_CONFIG=rockchip_rk356x_recovery
TARGET_PCBA_CONFIG=
TARGET_RAMBOOT_CONFIG=
============================================
============Start building uboot============
TARGET_UBOOT_CONFIG=rk3568
=========================================
## make rk3568_defconfig -j64
#
# configuration written to .config
#
scripts/kconfig/conf  --silentoldconfig Kconfig
  CHK     include/config.h
  GEN     include/autoconf.mk.dep
  CFG     u-boot.cfg
  CFG     spl/u-boot.cfg
  CFG     tpl/u-boot.cfg
  GEN     include/autoconf.mk
  GEN     spl/include/autoconf.mk
  GEN     tpl/include/autoconf.mk
  CHK     include/config/uboot.release
  CHK     include/generated/timestamp_autogenerated.h
  UPD     include/generated/timestamp_autogenerated.h
  CHK     include/generated/version_autogenerated.h
  CHK     include/generated/generic-asm-offsets.h
  CHK     include/generated/asm-offsets.h
  HOSTCC  tools/mkenvimage.o
  HOSTCC  tools/fit_image.o
  HOSTCC  tools/image-host.o
  HOSTCC  tools/mkimage.o
  HOSTCC  tools/dumpimage.o
  HOSTCC  tools/rockchip/boot_merger.o
  HOSTCC  tools/rockchip/loaderimage.o
tools/rockchip/boot_merger.c: In function ‘main’:
tools/rockchip/boot_merger.c:895:11: warning: array subscript 20 is outside array bounds of ‘char[20]’ [-Warray-bounds]
  895 |  str[len] = 0;
      |  ~~~~~~~~~^~~
tools/rockchip/boot_merger.c:933:7: note: while referencing ‘name’
  933 |  char name[MAX_NAME_LEN];
      |       ^~~~
  HOSTLD  tools/mkenvimage
  HOSTLD  tools/dumpimage
  HOSTLD  tools/mkimage
  HOSTLD  tools/boot_merger
  CHK     include/config.h
  CFG     u-boot.cfg
  HOSTLD  tools/loaderimage
  CC      arch/arm/cpu/armv8/fwcall.o
  LD      arch/arm/cpu/armv8/built-in.o
  CC      drivers/usb/gadget/f_fastboot.o
  CC      common/main.o
  CC      cmd/version.o
  LD      cmd/built-in.o
  LD      common/built-in.o
  CC      lib/display_options.o
  LD      lib/built-in.o
  LD      drivers/usb/gadget/built-in.o
  LD      u-boot
  OBJCOPY u-boot.srec
  OBJCOPY u-boot-nodtb.bin
  SYM     u-boot.sym
start=$(/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/prebuilts/gcc/linux-x86/aarch64/gcc-arm-10.3-2021.07-x86_64-aarch64-none-linux-gnu/bin/aarch64-none-linux-gnu-nm u-boot | grep __rel_dyn_start | cut -f 1 -d ' '); end=$(/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/prebuilts/gcc/linux-x86/aarch64/gcc-arm-10.3-2021.07-x86_64-aarch64-none-linux-gnu/bin/aarch64-none-linux-gnu-nm u-boot | grep __rel_dyn_end | cut -f 1 -d ' '); tools/relocate-rela u-boot-nodtb.bin 0x00a00000 $start $end
make[2]: 'arch/arm/dts/rk3568-evb.dtb' is up to date.
  COPY    u-boot.dtb
  CAT     u-boot-dtb.bin
  MKIMAGE u-boot.img
  MKIMAGE u-boot-dtb.img
  COPY    u-boot.bin
  ALIGN   u-boot.bin
  COPY    spl/u-boot-spl.dtb
  CC      tpl/arch/arm/mach-rockchip/tpl.o
  CC      spl/common/spl/spl.o
  CC      spl/arch/arm/cpu/armv8/fwcall.o
  CC      tpl/arch/arm/cpu/armv8/fwcall.o
  CC      spl/lib/display_options.o
  LD      spl/arch/arm/cpu/armv8/built-in.o
  LD      tpl/arch/arm/cpu/armv8/built-in.o
  LD      tpl/arch/arm/mach-rockchip/built-in.o
  LD      spl/common/spl/built-in.o
  LD      spl/lib/built-in.o
  LD      tpl/u-boot-tpl
  OBJCOPY tpl/u-boot-tpl-nodtb.bin
  COPY    tpl/u-boot-tpl.bin
  LD      spl/u-boot-spl
  OBJCOPY spl/u-boot-spl-nodtb.bin
  CAT     spl/u-boot-spl-dtb.bin
  COPY    spl/u-boot-spl.bin
  CFGCHK  u-boot.cfg
SEC=1
pack u-boot.itb okay! Input: ../rkbin/RKTRUST/RK3568TRUST.ini

FIT description: FIT Image with ATF/OP-TEE/U-Boot/MCU
Created:         Tue Nov 29 20:26:55 2022
 Image 0 (uboot)
  Description:  U-Boot
  Created:      Tue Nov 29 20:26:55 2022
  Type:         Standalone Program
  Compression:  uncompressed
  Data Size:    1282592 Bytes = 1252.53 KiB = 1.22 MiB
  Architecture: AArch64
  Load Address: 0x00a00000
  Entry Point:  unavailable
  Hash algo:    sha256
  Hash value:   76a4dd19889f241a14bcb5bdf72c9ce6b8779345bceae46f3e748c308b61d3ec
 Image 1 (atf-1)
  Description:  ARM Trusted Firmware
  Created:      Tue Nov 29 20:26:55 2022
  Type:         Firmware
  Compression:  uncompressed
  Data Size:    163840 Bytes = 160.00 KiB = 0.16 MiB
  Architecture: AArch64
  Load Address: 0x00040000
  Hash algo:    sha256
  Hash value:   df3dd620f7412cc7233d775405bead9f3323bb12a1c902dafd71752357211505
 Image 2 (atf-2)
  Description:  ARM Trusted Firmware
  Created:      Tue Nov 29 20:26:55 2022
  Type:         Firmware
  Compression:  uncompressed
  Data Size:    40960 Bytes = 40.00 KiB = 0.04 MiB
  Architecture: AArch64
  Load Address: 0xfdcc1000
  Hash algo:    sha256
  Hash value:   455304ad25a671f34193e732b2c3c679f4ef43d6254f642c29d1643c937cf2d9
 Image 3 (atf-3)
  Description:  ARM Trusted Firmware
  Created:      Tue Nov 29 20:26:55 2022
  Type:         Firmware
  Compression:  uncompressed
  Data Size:    20259 Bytes = 19.78 KiB = 0.02 MiB
  Architecture: AArch64
  Load Address: 0x0006a000
  Hash algo:    sha256
  Hash value:   919db4e965c19bf879da8a058ac6008a892a17904e6437cdd72f8f485aa61e0c
 Image 4 (atf-4)
  Description:  ARM Trusted Firmware
  Created:      Tue Nov 29 20:26:55 2022
  Type:         Firmware
  Compression:  uncompressed
  Data Size:    8192 Bytes = 8.00 KiB = 0.01 MiB
  Architecture: AArch64
  Load Address: 0xfdcd0000
  Hash algo:    sha256
  Hash value:   d4e8257343b8be878acde6ba7274e2e60640e5c20bffe754984761a31276b3de
 Image 5 (atf-5)
  Description:  ARM Trusted Firmware
  Created:      Tue Nov 29 20:26:55 2022
  Type:         Firmware
  Compression:  uncompressed
  Data Size:    8192 Bytes = 8.00 KiB = 0.01 MiB
  Architecture: AArch64
  Load Address: 0xfdcce000
  Hash algo:    sha256
  Hash value:   cb025e3a5b768cdea2ba62e092042d5194098016e43c323db954278ad7d75a84
 Image 6 (atf-6)
  Description:  ARM Trusted Firmware
  Created:      Tue Nov 29 20:26:55 2022
  Type:         Firmware
  Compression:  uncompressed
  Data Size:    7732 Bytes = 7.55 KiB = 0.01 MiB
  Architecture: AArch64
  Load Address: 0x00068000
  Hash algo:    sha256
  Hash value:   6e9d32ba2391ea86ec585080eebb4c76fae7b5363dca1a69e6035ba3e4491bc8
 Image 7 (optee)
  Description:  OP-TEE
  Created:      Tue Nov 29 20:26:55 2022
  Type:         Firmware
  Compression:  uncompressed
  Data Size:    457112 Bytes = 446.40 KiB = 0.44 MiB
  Architecture: AArch64
  Load Address: 0x08400000
  Hash algo:    sha256
  Hash value:   af414b9c9f1a05b058de55de4ad0fa6ec1f40e6b42769454196ee63279570cc7
 Image 8 (fdt)
  Description:  U-Boot dtb
  Created:      Tue Nov 29 20:26:55 2022
  Type:         Flat Device Tree
  Compression:  uncompressed
  Data Size:    14285 Bytes = 13.95 KiB = 0.01 MiB
  Architecture: AArch64
  Hash algo:    sha256
  Hash value:   fcfda359c09a8b315de67f0f6a4db29122f97fadfa185d0d4a9aee69488cc76d
 Default Configuration: 'conf'
 Configuration 0 (conf)
  Description:  rk3568-evb
  Kernel:       unavailable
  Firmware:     atf-1
  FDT:          fdt
  Loadables:    uboot
                atf-2
                atf-3
                atf-4
                atf-5
                atf-6
                optee
********boot_merger ver 1.2********
Info:Pack loader ok.
pack loader okay! Input: ../rkbin/RKBOOT/RK3568MINIALL.ini
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/u-boot

Image(no-signed, version=0): uboot.img (FIT with uboot, trust...) is ready
Image(no-signed): rk356x_spl_loader_v1.15.112.bin (with spl, ddr...) is ready
pack uboot.img okay! Input: ../rkbin/RKTRUST/RK3568TRUST.ini

Platform RK3568 is build OK, with new .config(make rk3568_defconfig -j64)
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/prebuilts/gcc/linux-x86/aarch64/gcc-arm-10.3-2021.07-x86_64-aarch64-none-linux-gnu/bin/aarch64-none-linux-gnu-
Tue Nov 29 20:26:56 CST 2022
Running build_uboot succeeded.
Skipping build_loader for missing configs:  RK_LOADER_BUILD_TARGET.
============Start building kernel============
TARGET_ARCH          =arm64
TARGET_KERNEL_CONFIG =rockchip_linux_defconfig
TARGET_KERNEL_DTS    =pro-rk3568
TARGET_KERNEL_CONFIG_FRAGMENT =
==========================================
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux
------ start build dtb------
------ end build dtb------
  CALL    scripts/checksyscalls.sh
  CHK     include/generated/compile.h
  Image:  kernel.img is ready
  CALL    scripts/checksyscalls.sh
  Building modules, stage 2.
  MODPOST 0 modules
  Image:  resource.img (with pro-rk3568.dtb logo.bmp logo_kernel.bmp) is ready
  Image1:  boot.img (with Image  resource.img) is ready
  Image2:  zboot.img (with Image.lz4  resource.img) is ready
Running build_kernel succeeded.
Skipping build_toolchain for missing configs:  RK_CFG_TOOLCHAIN.
==========Start building buildroot==========
TARGET_BUILDROOT_CONFIG=rockchip_rk3568
=========================================
Top of tree: /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux
===========================================

#TARGET_BOARD=rk3568
#OUTPUT_DIR=output/rockchip_rk3568
#CONFIG=rockchip_rk3568_defconfig

===========================================
make: Entering directory '/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot'
  GEN     /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/Makefile
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/build/defconfig_hook.py -m /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/configs/rockchip_rk3568_defconfig /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig
BR2_DEFCONFIG='' KCONFIG_AUTOCONFIG=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/build/buildroot-config/auto.conf KCONFIG_AUTOHEADER=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/build/buildroot-config/autoconf.h KCONFIG_TRISTATE=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/build/buildroot-config/tristate.config BR2_CONFIG=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.config HOST_GCC_VERSION="9" BASE_DIR=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568 SKIP_LEGACY= BR2_DEFCONFIG=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/configs/rockchip_rk3568_defconfig /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/build/buildroot-config/conf --defconfig=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig Config.in
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:259:warning: override: reassigning to symbol BR2_PACKAGE_ROCKCHIP_MPP
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:260:warning: override: reassigning to symbol BR2_PACKAGE_ROCKCHIP_MPP_ALLOCATOR_DRM
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:262:warning: override: reassigning to symbol BR2_PACKAGE_ROCKCHIP_RGA
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:287:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_GOOD_PLUGIN_RTP
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:288:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_GOOD_PLUGIN_RTPMANAGER
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:289:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_GOOD_PLUGIN_RTSP
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:295:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_BASE_PLUGIN_VIDEORATE
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:296:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_BASE_PLUGIN_VORBIS
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:297:warning: override: reassigning to symbol BR2_PACKAGE_GST1_PLUGINS_BASE_PLUGIN_OGG
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:300:warning: override: reassigning to symbol BR2_PACKAGE_BLUEZ5_UTILS
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:319:warning: override: reassigning to symbol BR2_PACKAGE_ROCKCHIP_TEST
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:322:warning: override: reassigning to symbol BR2_PACKAGE_RKWIFIBT
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.rockchipconfig:361:warning: override: reassigning to symbol BR2_PACKAGE_RKSCRIPT_IODOMAIN
#
# configuration written to /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/.config
#
make: Leaving directory '/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot'
2022-11-29T20:27:07 >>> python3 3.8.6 Extracting
2022-11-29T20:27:09 >>> python3 3.8.6 Patching
2022-11-29T20:27:09 >>> python3 3.8.6 Updating config.sub and config.guess
2022-11-29T20:27:09 >>> python3 3.8.6 Configuring
2022-11-29T20:27:09 >>> python3 3.8.6 Autoreconfiguring
2022-11-29T20:27:13 >>> python3 3.8.6 Patching libtool
2022-11-29T20:27:38 >>> python3 3.8.6 Building
2022-11-29T20:27:47 >>> python3 3.8.6 Installing to staging directory
2022-11-29T20:27:49 >>> python3 3.8.6 Fixing libtool files
2022-11-29T20:27:52 >>> python3 3.8.6 Installing to target
2022-11-29T20:27:57 >>>   Finalizing target directory
2022-11-29T20:28:06 >>>   Sanitizing RPATH in target tree
2022-11-29T20:28:22 >>>   Copying overlay board/rockchip/common/base
2022-11-29T20:28:22 >>>   Copying overlay board/rockchip/common/powermanager
2022-11-29T20:28:22 >>>   Copying overlay board/rockchip/rk356x/fs-overlay/
2022-11-29T20:28:22 >>>   Copying overlay board/rockchip/common/wifi
2022-11-29T20:28:22 >>>   Executing post-build script ../device/rockchip/common/post-build.sh
2022-11-29T20:28:22 >>>   Generating root filesystem image rootfs.cpio
2022-11-29T20:29:04 >>>   Generating root filesystem image rootfs.ext2
2022-11-29T20:29:08 >>>   Generating root filesystem image rootfs.squashfs
2022-11-29T20:29:11 >>>   Generating root filesystem image rootfs.tar
Done in 2min 11s
log saved on /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/br.log. pack buildroot image at: /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/images/rootfs.ext4
you take 2:11.64 to build builroot
Running build_buildroot succeeded.
Running build_rootfs succeeded.
==========Start building recovery==========
TARGET_RECOVERY_CONFIG=rockchip_rk356x_recovery
========================================
config is rockchip_rk356x_recovery
found kernel image
Top of tree: /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux
===========================================

#TARGET_BOARD=rk356x
#OUTPUT_DIR=output/rockchip_rk356x_recovery
#CONFIG=rockchip_rk356x_recovery_defconfig

===========================================
make: Entering directory '/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot'
  GEN     /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/Makefile
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/build/defconfig_hook.py -m /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/configs/rockchip_rk356x_recovery_defconfig /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/.rockchipconfig
BR2_DEFCONFIG='' KCONFIG_AUTOCONFIG=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/build/buildroot-config/auto.conf KCONFIG_AUTOHEADER=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/build/buildroot-config/autoconf.h KCONFIG_TRISTATE=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/build/buildroot-config/tristate.config BR2_CONFIG=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/.config HOST_GCC_VERSION="9" BASE_DIR=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery SKIP_LEGACY= BR2_DEFCONFIG=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/configs/rockchip_rk356x_recovery_defconfig /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/build/buildroot-config/conf --defconfig=/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/.rockchipconfig Config.in
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/.rockchipconfig:63:warning: override: reassigning to symbol BR2_PACKAGE_UPDATE
/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/.rockchipconfig:64:warning: override: reassigning to symbol BR2_PACKAGE_RKSCRIPT
#
# configuration written to /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/.config
#
make: Leaving directory '/home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot'
====Start build rockchip_rk356x_recovery====
2022-11-29T20:29:18 >>>   Finalizing target directory
2022-11-29T20:29:18 >>>   Sanitizing RPATH in target tree
2022-11-29T20:29:19 >>>   Copying overlay board/rockchip/common/base
2022-11-29T20:29:19 >>>   Copying overlay board/rockchip/common/recovery
2022-11-29T20:29:19 >>>   Copying overlay board/rockchip/rk356x/fs-overlay/
2022-11-29T20:29:19 >>>   Executing post-build script ../device/rockchip/common/post-build.sh
2022-11-29T20:29:19 >>>   Generating root filesystem image rootfs.cpio
2022-11-29T20:29:22 >>>   Generating root filesystem image rootfs.ext2
2022-11-29T20:29:24 >>>   Generating root filesystem image rootfs.squashfs
2022-11-29T20:29:24 >>>   Generating root filesystem image rootfs.tar
Done in 10s
log saved on /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/br.log
====Build rockchip_rk356x_recovery ok!====
pack recovery.img...fdt {
kernel {
ramdisk {
resource {
FIT description: U-Boot FIT source file for arm
Created:         Tue Nov 29 20:29:25 2022
 Image 0 (fdt)
  Description:  unavailable
  Created:      Tue Nov 29 20:29:25 2022
  Type:         Flat Device Tree
  Compression:  uncompressed
  Data Size:    134094 Bytes = 130.95 KiB = 0.13 MiB
  Architecture: AArch64
  Load Address: 0xffffff00
  Hash algo:    sha256
  Hash value:   e0892143708bd0c44ea74bf2eddda4ef0d8c2767bc9142976b37f1bb9f33a7ec
 Image 1 (kernel)
  Description:  unavailable
  Created:      Tue Nov 29 20:29:25 2022
  Type:         Kernel Image
  Compression:  uncompressed
  Data Size:    27842568 Bytes = 27190.01 KiB = 26.55 MiB
  Architecture: AArch64
  OS:           Linux
  Load Address: 0xffffff01
  Entry Point:  0xffffff01
  Hash algo:    sha256
  Hash value:   0ad323eb8ef84ca0eefe0c5f5991dbcf555d05d69c02c15db6b13db80d1c0246
 Image 2 (ramdisk)
  Description:  unavailable
  Created:      Tue Nov 29 20:29:25 2022
  Type:         RAMDisk Image
  Compression:  uncompressed
  Data Size:    10979148 Bytes = 10721.82 KiB = 10.47 MiB
  Architecture: AArch64
  OS:           Linux
  Load Address: 0xffffff02
  Entry Point:  unavailable
  Hash algo:    sha256
  Hash value:   28b68d3976726005119661698f789f4b22b039c77686332440e1cd2211e2f890
 Image 3 (resource)
  Description:  unavailable
  Created:      Tue Nov 29 20:29:25 2022
  Type:         Multi-File Image
  Compression:  uncompressed
  Data Size:    172032 Bytes = 168.00 KiB = 0.16 MiB
  Hash algo:    sha256
  Hash value:   3c761c0e0dc0cddfeb7566efeba5b1785567aa8618efed2b10066b90673ded3b
 Default Configuration: 'conf'
 Configuration 0 (conf)
  Description:  unavailable
  Kernel:       kernel
  Init Ramdisk: ramdisk
  FDT:          fdt
done.
you take 0:11.76 to build recovery
Running build_recovery succeeded.
Skipping build_ramboot for missing configs:  RK_CFG_RAMBOOT.
Running build_all succeeded.
/usr/bin/fakeroot
 Linking parameter.txt from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/device/rockchip/rk356x/parameter-buildroot-fit.txt... 
 Done linking parameter.txt 
 Linking uboot.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/u-boot/uboot.img... 
 Done linking uboot.img 
 Linking MiniLoaderAll.bin from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/u-boot/rk356x_spl_loader_v1.15.112.bin... 
 Done linking MiniLoaderAll.bin 
 Linking boot.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/kernel/boot.img... 
 Done linking boot.img 
 Linking recovery.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk356x_recovery/images/recovery.img... 
 Done linking recovery.img 
 Linking misc.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/device/rockchip/rockimg/misc.img... 
 Fallback to /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/device/rockchip/rockimg/wipe_all-misc.img 
 Done linking misc.img 
 Linking rootfs.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/rockdev/rootfs.ext4... 
 Done linking rootfs.img 
 Packing oem.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/device/rockchip/oem/oem_normal... 
Using host tools in /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/host
Making /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/rockdev/oem.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/device/rockchip/oem/oem_normal (auto sized)
Making /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/rockdev/oem.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/device/rockchip/oem/oem_normal with size(17048KB)
mke2fs 1.46.5 (30-Dec-2021)
Discarding device blocks: done                            
Creating filesystem with 17048 1k blocks and 4272 inodes
Filesystem UUID: b13bf34a-58ed-46b7-a6ee-39bf02939997
Superblock backups stored on blocks: 
	8193

Allocating group tables: done                            
Writing inode tables: done                            
Copying files into the device: done
Writing superblocks and filesystem accounting information: done

tune2fs 1.46.5 (30-Dec-2021)
Setting maximal mount count to -1
Setting interval between checks to 0 seconds
 Done packing oem.img 
 Packing userdata.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/device/rockchip/userdata/userdata_normal... 
Using host tools in /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/buildroot/output/rockchip_rk3568/host
Making /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/rockdev/userdata.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/device/rockchip/userdata/userdata_normal (auto sized)
Making /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/rockdev/userdata.img from /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/device/rockchip/userdata/userdata_normal with size(4376KB)
mke2fs 1.46.5 (30-Dec-2021)
Discarding device blocks: done                            
Creating filesystem with 4376 1k blocks and 1096 inodes

Allocating group tables: done                            
Writing inode tables: done                            
Copying files into the device: done
Writing superblocks and filesystem accounting information: done

tune2fs 1.46.5 (30-Dec-2021)
Setting maximal mount count to -1
Setting interval between checks to 0 seconds
 Done packing userdata.img 
 Images in /home/rpdzkj/ninth/yushun/rk3566-rk3568-linux/rockdev are ready! 
Running build_firmware succeeded.
Make update.img
start to make update.img...
Android Firmware Package Tool v2.0
------ PACKAGE ------
Add file: ./package-file
package-file,Add file: ./package-file done,offset=0x800,size=0x28d,userspace=0x1
Add file: ./Image/MiniLoaderAll.bin
bootloader,Add file: ./Image/MiniLoaderAll.bin done,offset=0x1000,size=0x709c0,userspace=0xe2
Add file: ./Image/parameter.txt
parameter,Add file: ./Image/parameter.txt done,offset=0x72000,size=0x1b9,userspace=0x1
Add file: ./Image/uboot.img
uboot,Add file: ./Image/uboot.img done,offset=0x72800,size=0x400000,userspace=0x800
Add file: ./Image/misc.img
misc,Add file: ./Image/misc.img done,offset=0x472800,size=0xc000,userspace=0x18
Add file: ./Image/boot.img
boot,Add file: ./Image/boot.img done,offset=0x47e800,size=0x1ab8800,userspace=0x3571
Add file: ./Image/recovery.img
recovery,Add file: ./Image/recovery.img done,offset=0x1f37000,size=0x2551a00,userspace=0x4aa4
Add file: ./Image/rootfs.img
rootfs,Add file: ./Image/rootfs.img done,offset=0x4489000,size=0x313a3000,userspace=0x62746
Add CRC...
Make firmware OK!
------ OK ------
********rkImageMaker ver 2.0********
Generating new image, please wait...
Writing head info...
Writing boot file...
Writing firmware...
Generating MD5 data...
MD5 data generated successfully!
New image generated successfully!
Making ./Image/update.img OK.
Running build_updateimg succeeded.
Running build_allsave succeeded.
